Pervious concrete

F.N.Jain\*,S.D.Indurkar\*,S.Paroche\*,(\*-final year,civil engg.,K.D.K.C.E)

Abstract

This paper describes the effect of size of aggregates and proportion of cement , aggregates, admixtures and water on porosity of Pervious Concrete which is the main feature of Pervious Conrete. It can be utilized for improving the ground water recharge and efficient water percolation on pavements. Different sample blocks were made in lab with variations in mixture to see the porosity for final conclusion.